
Open the V2.35 firmware.

Press and hold the "options" button on the steering wheel and then plug the steering wheel usb port into the computer, then click "Update" to update the firmware, and then read the bar after it is finished.

 This message is displayed to indicate that the update was successful