Open the firmware, hold down the “options” button on the game steering wheel without releasing it, then plug the steering wheel's USB port into the computer. Click 'Update' at this point to start the update process. After the progress bar completes, if the following image appears, the update is successful.

